[FTC CAD FILE LABELING SYSTEM]

Marcus Roberts

ANY SKETCHES BEFORE FILES ARE MADE:

Alpha V1

Alpha V2

|

V

Etc.

-------------------------------------------------------------------------------------------------------------------------------

CAD FILES

**[SAVE AS. NEVER SAVE OVER]**

Very first part design:

V1.0

Small changes and measurement fixes

V1.0.1

Larger structural changes

V1.1

Overhaul of original design [NOTE: OVERRIDES ALL OTHER CHANGES]

V2.0

[EXAMPLE]

A part that has had 4 small changes and measurement fixes, 5 larger structural changes, and THEN has an overhaul will still be known as V2.0

A part that has had an overhaul and THEN has 4 small changes and measurement fixes along with 5 larger structural changes will be known as V2.5.4

-------------------------------------------------------------------------------------------------------------------------------

Please keep every change made, large and small. This will keep a detailed history of your CAD efforts and synergizes with the labeling system put in place. A good CAD file will look something like this:

V1.0

V1.1

V1.2

V1.2.1

V1.2.2

V1.2.3

V1.2.4

V1.2.5

V1.3.5

V2.0

V2.0.1

V2.0.2